Version: V129904.324147 | Release Date: 2012-02-01

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Menus]

lcs+340
Vendor ID | 419 (0x01a3) |
Vendor Name | microsonic GmbH
Vendor Text | microsonic GmbH
Vendor URL | http://www.microsonic.de
Device ID | 8 (0x000008)
Communication
IO-Link Revision | V1.0
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 43.2 ms
SIO Mode Supported | yes
Device Variant | lcs+340/F
--- | ---
Description | Ultrasonic proximity switch with 1 push-pull switched output, loadable to 100 mA, 3500 mm operating range IODD is applicable to: lcs+340/F
Product ID | 340/F
Device Icon |
Device Symbol |

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "Interval, switching status" id=PD_ProcessDataIn

bit length: 16
data type: 16-bit Record

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 1 | 15-bit UInteger |  |  |  |  |  | Interval |
2 | 0 | Boolean | false = Not connected, true = Connected |  |  |  |  | Switching status |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 1
element bit | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 1 | 2
element bit | 6 | 5 | 4 | 3 | 2 | 1 | 0 |

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Frame Capability |
5 | 88 | 8-bit UInteger |  | 16 |  |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Reserved |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Reserved |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Offset Time |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Reserved |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Reserved |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "System Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 161 = Teach-in detect point, 162 = Teach-in detect point + 8 %, 163 = Teach-in window mode detect point 1, 164 = Teach-in window mode detect point 2, 165 = Teach-in two-way refelctive barrier, 166 = Reset to factory setting
access rights: wo

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "microsonic GmbH"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "www.microsonic.de"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
default value: "lcs+"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
default value: "340/F"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
default value: "Ultraschall-Sensor"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
default value: " "
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Hardware Version" index=22 id=V_HardwareRevision

data type: 64-octet String UTF-8
default value: "-"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
default value: "-"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

[Top]

## Variable "Detect point 1" index=64 id=V_SwitchPoint1

description: The switched output is activated when the distance to an object is under that of the preset detect point 1. Adjusting range: 350.05 … 4997.94 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution.
data type: 16-bit UInteger
allowed values: 2038..29098
default value: 19795
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Return detect point 1" index=65 id=V_BackspacePoint1

description: The switched output is reactivated when the distance to an object is greater than the preset return detect point 1 (detect point 1 + hysteresis). Adjusting range: 351.08 … 4998.97 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. The return detect point 1 must always be greater than the detect point 1.
data type: 16-bit UInteger
allowed values: 2044..29104
default value: 20086
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Detect point 2" index=66 id=V_SwitchPoint2

description: The switched output is activated when the distance to an object is under that of the preset detect point 2. Adjusting range: 351.94 … 9998.97 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. If the detect point 2 and the return detect point 2 are above the maximum range, window mode is disabled.
data type: 16-bit UInteger
allowed values: 2049..58214
default value: 58214
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Return detect point 2" index=67 id=V_BackspacePoint2

description: The switched output is reactivated when the distance to an object is greater than the preset return detect point 2 (detect point 2 + hysteresis). Adjusting range: 351.08 … 9998.97 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. The return detect point 2 must always be greater than the detect point 2. If the detect point 2 and the return detect point 2 are above the maximum range, window mode is disabled.
data type: 16-bit UInteger
allowed values: 2044..58214
default value: 58203
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Foreground suppression" index=68 id=V_Foregroundsupression

description: All echo signals closer than foreground suppression are ignored. Adjusting range: 318.96 … 1049.98 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. The foreground suppression is an offset on the blind zone
data type: 16-bit UInteger
allowed values: 0..4256
default value: 0
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Maximum range" index=69 id=V_DetectionRange

description: Maximum detection range of the sensor. Adjusting range: 318.96 … 9990.04 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution.
data type: 16-bit UInteger
allowed values: 29110..58162
default value: 29110
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Teach-in via push-button T1/T2" index=70 id=V_TeachButton

description: This function locks the push-buttons
data type: 8-bit UInteger
allowed values: 0 = Push-buttons are deactivated, 2 = Push-buttons are activated
default value: 2
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Set NOC/NCC" index=71 id=V_SwitchingMode

description: The NOC or NCC output function can be preset for the switched output.
data type: 8-bit UInteger
allowed values: 0 = NOC normally open, 2 = NCC normally closed
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Measurement filter" index=72 id=V_Filter

description: There are 5 filter settings: F00: No filter | F01: Standard filter | F02: Average value filter | F03: foreground filter | F04: background filter
data type: 8-bit UInteger
allowed values: 0 = F00, 1 = F01, 2 = F02, 3 = F03, 4 = F04
default value: 1
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Filter strength" index=73 id=V_FilterValue

description: A filter strength between 0 – weak filter effect – and 9 – pronounced filter effect – can be selected for each measurement filter.
data type: 8-bit UInteger
allowed values: 0 = P00, 1 = P01, 2 = P02, 3 = P03, 4 = P04, 5 = P05, 6 = P06, 7 = P07, 8 = P08, 9 = P09
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Temperature compensation" index=74 id=V_TempMode

description: The Temperature compensation may be activated or deactivated.
data type: 8-bit UInteger
allowed values: 0 = Temperature compensation is off, 1 = Temperature compensation is on
default value: 1
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Switch-on delay" index=75 id=V_SwitchOnDelay

description: The effect of the distance measured to an object falling under the preset detect point is for the change in the state at the switched output to be delayed for the selected time. Pointer: if the distance to the object increases over the detect point again, the switches output is set back after 50 % of the set switch-on delay time. Adjusting range: 1...20 s
data type: 8-bit UInteger
allowed values: 0 = Deactivated, 1 = 1, 2 = 2, 3 = 3, 4 = 4, 5 = 5, 6 = 6, 7 = 7, 8 = 8, 9 = 9, 10 = 10, 11 = 11, 12 = 12, 13 = 13, 14 = 14, 15 = 15, 16 = 16, 17 = 17, 18 = 18, 19 = 19, 20 = 20
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Detection zone sensivity" index=76 id=V_Sensivity

description: Affects the size of the detection zone. There are 3 sensitivity settings: E01: sensivity is high | E02: sensivity is standard | E03: sensivity is low
data type: 8-bit UInteger
allowed values: 1 = E01: sensivity is high, 2 = E02: sensivity is standard, 3 = E03: sensivity is low
default value: 2
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Multiplex mode device addressing" index=77 id=V_AdressMultiplex

description: For synchronisation and multiplex mode the Sync-channels (Pin 5 at the sensors receptacle) of all sensores (10 maximum) have to be connected. Additionally an individual device address from 01 to 10 can be assigned. The sensors perform the ultrasonic measurement sequentially from low to high address. Therefor any influence between the sensors is rejected. To use synchronized mode all sensors must be set to address 00
data type: 8-bit UInteger
allowed values: 0 = Synchronisation is on, 1 = Multiplex Mode with adress 01, 2 = Multiplex Mode with adress 02, 3 = Multiplex Mode with adress 03, 4 = Multiplex Mode with adress 04, 5 = Multiplex Mode with adress 05, 6 = Multiplex Mode with adress 06, 7 = Multiplex Mode with adress 07, 8 = Multiplex Mode with adress 08, 9 = Multiplex Mode with adress 09, 10 = Multiplex Mode with adress 10, 11 = Synchronisation is off
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Multiplex mode highest address" index=78 id=V_MaxAdressMultiplex

description: To optimize the multiplex speed the highest sensor address may be set. Adjusting range: 01...10
data type: 8-bit UInteger
allowed values: 1 = Highest address 1, 2 = Highest address 2, 3 = Highest address 3, 4 = Highest address 4, 5 = Highest address 5, 6 = Highest address 6, 7 = Highest address 7, 8 = Highest address 8, 9 = Highest address 9, 10 = Highest address 10
default value: 10
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Interference noise suppression" index=79 id=V_NoiseSuppression

description: The interference noise suppressor detects and shunts out interference which may, for instance, be caused by compressed air. The state of the switched output is frozen during the interference.
data type: 8-bit UInteger
allowed values: 0 = Deactivated, 1 = Activated
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Echo Quality" index=80 id=V_Quality

description: Adjust the sensor, so that the value of the Echo quality reaches the maximum.
data type: 16-bit UInteger
default value: 0
access rights: ro

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Distance value" index=81 id=V_PD

description: The measured distance value is output with a resolution of 1 mm.
data type: 16-bit UInteger
default value: 5000
access rights: ro

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
25424 (0x6350) | Message | Parameter changed | Parameter changed
36000 (0x8ca0) | Message | Teach in failed | Teach in failed

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText

Observation Menu
V_SwitchPoint1 * 0.1717623 + 0 mm, ro
V_BackspacePoint1 * 0.1717623 + 0 mm, ro
V_BackspacePoint2 * 0.1717623 + 0 mm, ro
V_SwitchPoint2 * 0.1717623 + 0 mm, ro
V_Foregroundsupression * 0.1717623 + 319 mm, ro
V_DetectionRange * 0.1717623 + 0 mm, ro
V_SwitchingMode, ro
V_TeachButton
V_Filter, ro
V_FilterValue, ro
V_TempMode, ro
V_SwitchOnDelay s, ro
V_Sensivity, ro
V_AdressMultiplex, ro
V_MaxAdressMultiplex, ro
V_NoiseSuppression, ro
V_Quality, ro
V_PD, ro

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_HardwareRevision
V_FirmwareRevision

Parameter Menu
V_SwitchPoint1 * 0.1717623 + 0 mm
V_BackspacePoint1 * 0.1717623 + 0 mm
V_BackspacePoint2 * 0.1717623 + 0 mm
V_SwitchPoint2 * 0.1717623 + 0 mm
V_SwitchingMode
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
V_SystemCommand, Button:=165
V_SystemCommand, Button:=166

Observation Menu
V_Filter, ro
V_FilterValue, ro
V_SwitchOnDelay s, ro
V_NoiseSuppression, ro
V_Quality, ro
V_PD, ro

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_HardwareRevision
V_FirmwareRevision

Parameter Menu
V_SwitchPoint1 * 0.1717623 + 0 mm
V_BackspacePoint1 * 0.1717623 + 0 mm
V_BackspacePoint2 * 0.1717623 + 0 mm
V_SwitchPoint2 * 0.1717623 + 0 mm
V_Foregroundsupression * 0.1717623 + 319 mm
V_DetectionRange * 0.1717623 + 0 mm
V_SwitchingMode
V_TeachButton
V_Filter
V_FilterValue
V_TempMode
V_SwitchOnDelay s
V_Sensivity
V_AdressMultiplex
V_MaxAdressMultiplex
V_NoiseSuppression
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
V_SystemCommand, Button:=165
V_SystemCommand, Button:=166

Observation Menu
V_Quality, ro
V_PD, ro

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.