Version: V107823.496567 | Release Date: 2016-05-13

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Menus]

pico+25
Vendor ID | 419 (0x01a3) |
Vendor Name | microsonic GmbH
Vendor Text | microsonic GmbH
Vendor URL | http://www.microsonic.de
Device ID | 1 (0x000001)
Communication
IO-Link Revision | V1.0
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 8.4 ms
SIO Mode Supported | yes
Device Variant | pico+25/F
--- | ---
Description | Ultrasonic proximity switch with 1 push-pull switched output, loadable to 100 mA, 250 mm operating range IODD is applicable to: pico+25/F and pico+25/WK/F with angular head
Product ID | 25/F
Device Icon |
Device Symbol |
Device Variant | pico+25/WK/F
Description | Ultrasonic proximity switch with 1 push-pull switched output, loadable to 100 mA, 250 mm operating range IODD is applicable to: pico+25/F and pico+25/WK/F with angular head
Product ID | 25/WK/F
Device Icon |
Device Symbol |

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "Interval, switching status" id=PD_ProcessDataIn

bit length: 16
data type: 16-bit Record

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 1 | 15-bit UInteger |  |  |  |  |  | Interval |
2 | 0 | Boolean | false = Not connected, true = Connected |  |  |  |  | Switching status |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 1
element bit | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 1 | 2
element bit | 6 | 5 | 4 | 3 | 2 | 1 | 0 |

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Frame Capability |
5 | 88 | 8-bit UInteger |  | 16 |  |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Reserved |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Reserved |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Offset Time |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Reserved |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Reserved |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "System Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 161 = Teach one switch point, 162 = Teach switch point 8% behind object, 164 = Teach two-way barrier, 168 = Load factory settings
access rights: wo

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "microsonic GmbH"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "www.microsonic.de"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
default value: "pico+"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
default value: "25/F"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
default value: "Ultraschall-Sensor"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Hardware Version" index=22 id=V_HardwareRevision

data type: 64-octet String UTF-8
default value: "-"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
default value: "-"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

[Top]

## Variable "Detect point 1" index=64 id=V_SwitchPoint1

description: The switched output is activated when the distance to an object is under that of the preset detect point. Adjusting range: 30.1 ... 347.9 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution.
data type: 16-bit UInteger
allowed values: 436..5065
default value: 3639
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Return detect point 1" index=65 id=V_BackspacePoint1

description: The switched output is reactivated when the distance to an object is greater than the preset return detect point (detect point +hysteresis). Adjusting range: 31.1 ... 348.9 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. The return detect point must always be greater than the detect point.
data type: 16-bit UInteger
allowed values: 451..5080
default value: 3682
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "NO/NC operation" index=66 id=V_SwitchingMode

description: The NC or NO output function can be preset for the switched output.
data type: 8-bit UInteger
allowed values: 0 = NO normally open, 2 = NC normally closed
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Filter" index=67 id=V_Filter

description: There are 3 filter settings: F00: No filter | F01: Standard filter | F02: Average value filter
data type: 8-bit UInteger
allowed values: 0 = F00, 1 = F01, 2 = F02
default value: 1
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Filter strength" index=68 id=V_FilterValue

description: A filter strength between 0 – weak filter effect – and 9 – pronounced filter effect – can be selected for each measurement filter.
data type: 8-bit UInteger
allowed values: 0 = P00, 1 = P01, 2 = P02, 3 = P03, 4 = P04, 5 = P05, 6 = P06, 7 = P07, 8 = P08, 9 = P09
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Detect point 2" index=71 id=V_SwitchPoint2

description: The switched output is activated when the distance to an object is under that of the preset detect point. Adjusting range: 32.1 ... 349.9 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. If the switchpoint 2 and the return detect point 2 are above the maximum range, window mode is disabled.
data type: 16-bit UInteger
allowed values: 466..65512
default value: 65512
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Return detect point 2" index=72 id=V_BackspacePoint2

description: The switched output is reactivated when the distance to an object is greater than the preset return detect point (detect point +hysteresis). Adjusting range: 31.1 ... 348.9 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. The return detect point must always be greater than the detect point. If the switchpoint 2 and the return detect point 2 are above the maximum range, window mode is disabled.
data type: 16-bit UInteger
allowed values: 451..65512
default value: 65512
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Foreground supression" index=73 id=V_Foregroundsupression

description: All echo signals closer than foreground supression are ignored. Adjusting range: 27 ... 250 mm Pointer: The entered value is rounded to a multiple of the measurement value resolution. The foreground supression is an offset on the blindzone
data type: 16-bit UInteger
allowed values: 0..3246
default value: 0
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Teach in via pin 5" index=74 id=V_Ext_Teach

description: Activate/Deactivate external teach in via pin 5 Pointer: Teach in via Pin 5 is available only in SIO mode. During IO-Link mode pin 5 has no function.
data type: 8-bit UInteger
allowed values: 0 = Activated, 16 = Deactivated
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
25424 (0x6350) | Message | Parameter changed |
36000 (0x8ca0) | Message | Teach in failed |

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText

Observation Menu
V_SwitchPoint1 * 0.06870491 + 0 mm, ro
V_BackspacePoint1 * 0.06870491 + 0 mm, ro
V_SwitchPoint2 * 0.06870491 + 0 mm, ro
V_BackspacePoint2 * 0.06870491 + 0 mm, ro
V_Foregroundsupression * 0.06870491 + 27 mm, ro
V_SwitchingMode, ro
V_Filter, ro
V_FilterValue, ro
V_Ext_Teach, ro

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_HardwareRevision
V_FirmwareRevision

Parameter Menu
V_SwitchPoint1 * 0.06870491 + 0 mm
V_BackspacePoint1 * 0.06870491 + 0 mm
V_SwitchPoint2 * 0.06870491 + 0 mm
V_BackspacePoint2 * 0.06870491 + 0 mm
V_Foregroundsupression * 0.06870491 + 27 mm
V_SwitchingMode
V_SystemCommand, Button:=164
V_SystemCommand, Button:=168
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162

Observation Menu
V_Filter, ro
V_FilterValue, ro
V_Ext_Teach, ro

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_HardwareRevision
V_FirmwareRevision

Parameter Menu
V_SwitchPoint1 * 0.06870491 + 0 mm
V_BackspacePoint1 * 0.06870491 + 0 mm
V_SwitchPoint2 * 0.06870491 + 0 mm
V_BackspacePoint2 * 0.06870491 + 0 mm
V_Foregroundsupression * 0.06870491 + 27 mm
V_SwitchingMode
V_Filter
V_FilterValue
V_Ext_Teach
V_SystemCommand, Button:=164
V_SystemCommand, Button:=168
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.