Version: V210723.805614 | Release Date: 2022-11-25

[Process Data]
[Standard Variables]
[Variables]
[ErrorTypes]
[Events]
[Process Data Formatting]
[Menus]

nano-15/CF
Vendor ID | 419 (0x01a3) |
Vendor Name | microsonic GmbH
Vendor Text | Unser Herz schallt ultra.
Vendor URL | https://www.microsonic.de
Device ID | 85 (0x000055)
DeviceFamily | nano
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x0001 (Device Profile: Smart Sensor), 0x000a (Device Profile: ?Unknown?), 0x8000 (Function Class: Device Identification), 0x8001 (Function Class: Binary Data Channel), 0x8003 (Function Class: Device Diagnosis), 0x8004 (Function Class: Teach-In Commands), 0x800a (Function Class: ?Unknown?)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: no
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 8 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_1_2 with 2 octets on-request data OPERATE = TYPE_2_V with 1 octet on-request data ISDU supported
Device Variant | nano-15/CF
--- | ---
Description | Ultrasonic sensor in M12 brass sleeve, 1 push-pull switching output, 20 - 250 mm measuring range, 20 mm blindzone, 150 mm operating range, temperature compensation
Product ID | 34020
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Symbol |
- pin 1 | brown; L+
- pin 2 | white; NC; Com
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "Process data" id=PI_PDI32_MSDC32

bit length: 32
data type: 32-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 16-bit Integer | -32760 = Out of measuring range (-), 32760 = Out of measuring range (+), 32764 = No measurement data, 0..32000 |  |  |  |  | Process data value |
2 | 8 | 8-bit Integer |  |  |  |  |  | Process data scale |
3 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Switch signal channel 1 state |

Octet 0

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 1
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 1
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 2
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 3

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 3

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 65 = SP1 single value teach-in, 66 = SP2 single value teach-in, 130 = Restore Factory Settings |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 65 = SP1 single value teach-in, 66 = SP2 single value teach-in, 130 = Restore Factory Settings
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  | false |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  | false |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "microsonic GmbH"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "Unser Herz schallt ultra."
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
default value: "nano-15/CF"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
default value: "34020"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
default value: "Ultrasonic sensor"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Hardware Version" index=22 id=V_HardwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
default value: "***"
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Error Count" index=32 id=V_ErrorCount

data type: 16-bit UInteger
access rights: ro
dynamic

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure, 5..255 = Reserved
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

data type: Array[10] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48
subindex | 6 | 6 | 7 | 7 | 7 | 8 | 8 | 8

octet | 24 | 25 | 26 | 27 | 28 | 29 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 9 | 9 | 9 | 10 | 10 | 10 |

## Standard Variable "Process Data Input" index=40 id=V_ProcessDataInput

data type: see ProcessDataIn!
access rights: ro
dynamic
[Top]

## Variable "Teach-in channel" index=58 id=V_SSP_TI_TeachSelect

description: Choice of channel for the next teach-in procedure
data type: 8-bit UInteger
allowed values: 0 = SSC1: pin 4 (push-pull) (default), 1 = SSC1: pin 4 (push-pull)
default value: 0
access rights: rw
excluded from data storage

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Teach-in Result" index=59 id=V_SSP_TI_TeachResult

data type: 8-bit Record (subindex access not supported)
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Idle, 1 = SP1 success, 2 = SP2 success, 3 = SP12 success, 4 = Wait for command, 5 = Busy, 7 = Error | 0 |  |  |  | Teach-in status |

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1
element bit |  |  |  |  | 3 | 2 | 1 | 0

## Variable "SSC1 parameter" index=60 id=V_SSP_SSC01_Param

data type: 32-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 16-bit Integer | 200..2500 | 1500 |  |  |  | SP1 | Setpoint 1 for switching output
2 | 0 | 16-bit Integer | 200..2500 | 1700 |  |  |  | SP2 | Setpoint 2 for switching output

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 2 | 2 |
element bit | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "SSC1 configuration" index=61 id=V_SSP_SSC01_Config

data type: 32-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 8-bit UInteger | 0 = High active, 1 = Low active | 0 |  |  |  | Logic | Logic state for target detected
2 | 16 | 8-bit UInteger | 0 = Deactivated, 1 = Single point (SP1: switching point), 2 = Window (SP1, SP2: window mode), 3 = Two point (SP1, SP2: hysteresis mode), 128 = Single point + set point offset (SP1: switching point + offset), 129 = Window ± set point offset (SP1: two way reflective barrier) | 1 |  |  |  | Mode | Operation mode of the switch signal channel: switching point, window mode, hysteresis mode, switching point + offset, two way reflective barrier
3 | 0 | 16-bit UInteger | 10..2300 | 20 |  |  |  | Hysteresis | Hysteresis for SP1 and SP2

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "SSC1 advanced configuration" index=100 id=V_SSC01_AdvancedConfig

data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-on delay | Switch-on delay in seconds
2 | 8 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-off delay | Switch-off delay in seconds
3 | 0 | 8-bit UInteger | 2..20 | 8 |  |  |  | Set point offset | Offset value in % of SP1, which will be added to or subtracted from SP1.

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Measurement configuration" index=200 id=V_Messkonfig

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 16-bit Integer | 200..600 | 200 |  |  |  | Foreground suppression | The start of the measurement evaluation will be shifted from the blind zone to the value of the foreground suppression.

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 1 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Sound field width & Sensitivity" index=220 id=V_Empfindlichkeit

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0 = Narrow & Low, 1 = Normal & Standard, 2 = Wide & High | 2 |  |  |  | Amplifier setting |
2 | 0 | 8-bit UInteger | 0 = Inactive, 1 = Active | 0 |  |  |  | Sensibility hysteresis |

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Filter" index=256 id=V_Filter

data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 8-bit UInteger | 0 = F00: no filter, 1 = F01: standard filter, 2 = F02: averaging filter, 3 = F03: foreground filter, 4 = F04: background filter | 1 |  |  |  | Type | Measurement filter for the evaluation of the measured values
2 | 8 | 8-bit UInteger | 0 = P00: weak filter, 1 = P01, 2 = P02, 3 = P03, 4 = P04, 5 = P05, 6 = P06, 7 = P07, 8 = P08, 9 = P09: strong filter | 0 |  |  |  | Strength | Strength of the chosen measurement filter
3 | 0 | 8-bit Integer | 10..25 | 25 |  |  |  | Maximum object speed | Maximum object speed for a movement towards and away from the sensor. Valid (only) for type F01 and F02.

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Temperature compensation" index=300 id=V_TempKomp

description: The sensor is equipped with an internal temperature unit in order to determine the ambient temperature. Thus the temperature dependency of the sound velocity in air is compensated.
data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0 = fixed Value, 1 = Internal Temperatureprobe | 1 |  |  |  | Source | Evaluate the data of the internal temperature unit or use the reference temperature.
2 | 0 | 8-bit Integer | -25..70 | 20 |  |  |  | fixed Value | Is the internal temperature unit deactivited, the temperature compensation is using the reference temperature.

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Synchronisation and multiplex operation" index=350 id=V_SyncMux

data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 8-bit UInteger | 0 = Inactive, 1 = Active | 1 |  |  |  | Mode |
2 | 8 | 8-bit UInteger | 0 = Synchronisation active, 1 = Multiplex address 1, 2 = Multiplex address 2, 3 = Multiplex address 3, 4 = Multiplex address 4, 5 = Multiplex address 5, 6 = Multiplex address 6, 7 = Multiplex address 7, 8 = Multiplex address 8, 9 = Multiplex address 9, 10 = Multiplex address 10, 128 = IO-Link synchronisation active | 0 |  |  |  | Sensor operation |
3 | 0 | 8-bit UInteger | 2 = 2 participants, 3 = 3 participants, 4 = 4 participants, 5 = 5 participants, 6 = 6 participants, 7 = 7 participants, 8 = 8 participants, 9 = 9 participants, 10 = 10 participants | 10 |  |  |  | Multiplex number of participants | Maximum number of multiplex participants should be adjusted to correct number of participants in order to speed up multiplex operation.

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Pin 2" index=370 id=V_BedienungEingabe

data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Inactive, 1 = Active | 1 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "LED" index=371 id=V_BedienungAusgabe

data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Inactive, 1 = Active | 1 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Temperature compensation diagnosis" index=2000 id=V_DiagnoseTemperatur

data type: 24-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 16-bit Integer |  | 200 |  |  |  | Sensor temperature |
2 | 0 | 8-bit UInteger | 0 = Not completed, 1 = Completed | 0 |  |  |  | Heating-up phase |

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 2 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "Measurement data channel description" index=16512 id=V_SSP_MDC_Descriptor

data type: 88-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 56 | 32-bit Integer |  | 200 |  |  |  | Lower limit | Lower limit of the measuring range (blind zone)
2 | 24 | 32-bit Integer |  | 2500 |  |  |  | Upper limit | Upper limit of the measuring range (maximum range)
3 | 8 | 16-bit UInteger |  | 1013 |  |  |  | Unit code | IO-Link unit code: 1013 = [mm]
4 | 0 | 8-bit Integer |  | -1 |  |  |  | Scale | Process data value * (10 ^ scale) [Unit code] = measuring value in mm

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 4 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

[Top]

## ErrorTypes

Code | Additional code | Name | Description
--- | --- | --- | ---
129 (0x81) | 0 (0x00) | Parameter SP1 cannot be teached/set under VGA. |
129 (0x81) | 1 (0x01) | Parameter SP2 cannot be teached/set under VGA. |
129 (0x81) | 2 (0x02) | Parameter SP1 cannot be teached/set above GT. |
129 (0x81) | 3 (0x03) | Parameter SP2 cannot be teached/set above GT. |
129 (0x81) | 4 (0x04) | Parameter SP1 cannot be teached/set above GT - HY. |
129 (0x81) | 5 (0x05) | Parameter SP2 cannot be teached/set above GT - HY. |
129 (0x81) | 6 (0x06) | Parameter SP1 cannot be teached/set under VGA + HY. |
129 (0x81) | 7 (0x07) | Parameter SP2 cannot be teached/set under VGA + HY. |
129 (0x81) | 8 (0x08) | The distance between parameters SP1 and SP2 must be at least 2x hysteresis. |
129 (0x81) | 9 (0x09) | Parameter SP1 cannot be teached/set above GT - HY - Offset. |
129 (0x81) | 10 (0x0a) | Parameter SP1 cannot be teached/set under VGA + HY + Offset. |
129 (0x81) | 11 (0x0b) | The distance between parameters SP1 and SP2 must be at least 1 mm. |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
16384 (0x4000) | Error | Temperature fault | Overload
16912 (0x4210) | Warning | Device temperature over-run | Clear source of heat
16928 (0x4220) | Warning | Device temperature under-run | Insulate device
20736 (0x5100) | Error | General power supply fault | Check availability
30480 (0x7710) | Error | Short circuit | Check installation
36000 (0x8ca0) | Notification | Teach-in error | Teach-in process was not successful.
36001 (0x8ca1) | Notification | Teach-in success | Teach-in process was successful.
36002 (0x8ca2) | Notification | CycleTime error | CycleTime error is triggered if cycle time does not correspond to the permitted configuration.

[Top]

## Process Data Formatting

Formatting for Process Data id=PI_PDI32_MSDC32
Subindex 1: * 0.1 + 0 mm Dec.1
Subindex 2: * 1 + 0 Dec.0
Subindex 3:

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_HardwareRevision
V_ApplicationSpecificTag, rw

Observation Menu
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSP_SSC01_Param.SP1 * 0.1 + 0 mm, ro Dec.1
V_SSP_SSC01_Param.SP2 * 0.1 + 0 mm, ro Dec.1
V_SSP_SSC01_Config.Logic, ro
V_SSP_SSC01_Config.Mode, ro
V_SSP_SSC01_Config.Hysteresis * 0.1 + 0 mm, ro Dec.1
V_SSC01_AdvancedConfig.Switch-on delay * 0.1 + 0 s, ro Dec.1
V_SSC01_AdvancedConfig.Switch-off delay * 0.1 + 0 s, ro Dec.1
V_SSC01_AdvancedConfig.Set point offset * 1 + 0 %, ro Dec.0
Measurement configuration
V_Messkonfig.Foreground suppression * 0.1 + 0 mm, ro Dec.1
Filter
V_Filter.Type, ro
V_Filter.Strength, ro
V_Filter.Maximum object speed * 0.1 + 0 m/s, ro Dec.1
Temperature compensation
V_TempKomp.Source, ro
V_TempKomp.fixed Value * 1 + 0 °C, ro Dec.0
Sound field width & Sensitivity
V_Empfindlichkeit.Amplifier setting, rw
V_Empfindlichkeit.Sensibility hysteresis, rw
Synchronisation and multiplex operation
V_SyncMux.Mode, ro
V_SyncMux.Sensor operation, ro
V_SyncMux.Multiplex number of participants, ro
User interface
V_BedienungEingabe.Mode, ro
V_BedienungAusgabe.Mode, ro
Temperature compensation diagnosis
V_DiagnoseTemperatur.Sensor temperature * 0.1 + 0 °C, ro Dec.1
V_DiagnoseTemperatur.Heating-up phase, ro
ProcessDataInput
V_ProcessDataInput.1 * 0.1 + 0 mm, ro Dec.1
V_ProcessDataInput.2, ro Dec.0
V_ProcessDataInput.3, ro

Diagnosis Menu
Device status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus
Measurement data channel description
V_SSP_MDC_Descriptor.Lower limit * 0.1 + 0 mm, ro Dec.1
V_SSP_MDC_Descriptor.Upper limit * 0.1 + 0 mm, ro Dec.1
V_SSP_MDC_Descriptor.Unit code, ro
V_SSP_MDC_Descriptor.Scale, ro

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_HardwareRevision
V_ApplicationSpecificTag, rw

Parameter Menu
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSP_SSC01_Param.SP1 * 0.1 + 0 mm, rw Dec.1
V_SSP_SSC01_Param.SP2 * 0.1 + 0 mm, rw Dec.1
V_SSP_SSC01_Config.Logic, rw
V_SSP_SSC01_Config.Mode, rw
V_SSP_SSC01_Config.Hysteresis * 0.1 + 0 mm, rw Dec.1
V_SSC01_AdvancedConfig.Switch-on delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Switch-off delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Set point offset * 1 + 0 %, rw Dec.0
Teach-in channel
V_SystemCommand, Button:=65
V_SystemCommand, Button:=66
V_SSP_TI_TeachResult
Measurement configuration
V_Messkonfig.Foreground suppression * 0.1 + 0 mm, rw Dec.1
Filter
V_Filter.Type, rw
V_Filter.Strength, rw
V_Filter.Maximum object speed * 0.1 + 0 m/s, rw Dec.1
Temperature compensation
V_TempKomp.Source, rw
V_TempKomp.fixed Value * 1 + 0 °C, rw Dec.0
Sound field width & Sensitivity
V_Empfindlichkeit.Amplifier setting, rw
V_Empfindlichkeit.Sensibility hysteresis, rw
Synchronisation and multiplex operation
V_SyncMux.Mode, rw
V_SyncMux.Sensor operation, rw
V_SyncMux.Multiplex number of participants, rw
User interface
V_BedienungEingabe.Mode, rw
V_BedienungAusgabe.Mode, rw
System command
V_SystemCommand, Button:=130
Device access locks
V_DeviceAccessLocks.Parameter (write) Access Lock, rw
V_DeviceAccessLocks.Local Parameterization Lock, rw

Observation Menu
Temperature compensation diagnosis
V_DiagnoseTemperatur.Sensor temperature * 0.1 + 0 °C, ro Dec.1
V_DiagnoseTemperatur.Heating-up phase, ro
ProcessDataInput
V_ProcessDataInput.1 * 0.1 + 0 mm, ro Dec.1
V_ProcessDataInput.2, ro Dec.0
V_ProcessDataInput.3, ro

Diagnosis Menu
Device status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus
Measurement data channel description
V_SSP_MDC_Descriptor.Lower limit * 0.1 + 0 mm, ro Dec.1
V_SSP_MDC_Descriptor.Upper limit * 0.1 + 0 mm, ro Dec.1
V_SSP_MDC_Descriptor.Unit code, ro
V_SSP_MDC_Descriptor.Scale, ro

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_HardwareRevision
V_ApplicationSpecificTag, rw

Parameter Menu
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSP_SSC01_Param.SP1 * 0.1 + 0 mm, rw Dec.1
V_SSP_SSC01_Param.SP2 * 0.1 + 0 mm, rw Dec.1
V_SSP_SSC01_Config.Logic, rw
V_SSP_SSC01_Config.Mode, rw
V_SSP_SSC01_Config.Hysteresis * 0.1 + 0 mm, rw Dec.1
V_SSC01_AdvancedConfig.Switch-on delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Switch-off delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Set point offset * 1 + 0 %, rw Dec.0
Teach-in channel
V_SystemCommand, Button:=65
V_SystemCommand, Button:=66
V_SSP_TI_TeachResult
Measurement configuration
V_Messkonfig.Foreground suppression * 0.1 + 0 mm, rw Dec.1
Filter
V_Filter.Type, rw
V_Filter.Strength, rw
V_Filter.Maximum object speed * 0.1 + 0 m/s, rw Dec.1
Temperature compensation
V_TempKomp.Source, rw
V_TempKomp.fixed Value * 1 + 0 °C, rw Dec.0
Sound field width & Sensitivity
V_Empfindlichkeit.Amplifier setting, rw
V_Empfindlichkeit.Sensibility hysteresis, rw
Synchronisation and multiplex operation
V_SyncMux.Mode, rw
V_SyncMux.Sensor operation, rw
V_SyncMux.Multiplex number of participants, rw
User interface
V_BedienungEingabe.Mode, rw
V_BedienungAusgabe.Mode, rw
System command
V_SystemCommand, Button:=130
Device access locks
V_DeviceAccessLocks.Parameter (write) Access Lock, rw
V_DeviceAccessLocks.Local Parameterization Lock, rw

Observation Menu
Temperature compensation diagnosis
V_DiagnoseTemperatur.Sensor temperature * 0.1 + 0 °C, ro Dec.1
V_DiagnoseTemperatur.Heating-up phase, ro
ProcessDataInput
V_ProcessDataInput.1 * 0.1 + 0 mm, ro Dec.1
V_ProcessDataInput.2, ro Dec.0
V_ProcessDataInput.3, ro

Diagnosis Menu
Device status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus
Measurement data channel description
V_SSP_MDC_Descriptor.Lower limit * 0.1 + 0 mm, ro Dec.1
V_SSP_MDC_Descriptor.Upper limit * 0.1 + 0 mm, ro Dec.1
V_SSP_MDC_Descriptor.Unit code, ro
V_SSP_MDC_Descriptor.Scale, ro

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.