Version: V211861.840248 | Release Date: 2023-09-18

[Process Data]
[Standard Variables]
[Variables]
[ErrorTypes]
[Events]
[Process Data Formatting]
[Menus]

cube-340/FFIU
Vendor ID | 419 (0x01a3) |
Vendor Name | microsonic GmbH
Vendor Text | Unser Herz schallt ultra.
Vendor URL | https://www.microsonic.de
Device ID | 92 (0x00005c)
DeviceFamily | cube
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x0010 (Device Profile: ?Unknown?), 0x4000 (Common Application Profile: ?Unknown?)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: no
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 41.6 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_1_2 with 2 octets on-request data OPERATE = TYPE_2_V with 8 octets on-request data ISDU supported
Device Variant | cube-340/FFIU
--- | ---
Description | Ultrasonic sensor in cubic plastic housing, 2 push-pull switching and 1 analogue output 0-10 V/4..20 mA , 350 - 5000 mm measuring range, 350 mm blindzone, 3400 mm operating range, temperature compensation
Product ID | 43440
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
Connection Symbol |
- pin 1 | brown; L+
- pin 2 | white; Other; Push-Pull/Current/Voltage
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC; Com

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "Process data" id=PI_PDI32_MSDC32

bit length: 32
data type: 32-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 16-bit Integer | -32760 = Out of measuring range (-), 32760 = Out of measuring range (+), 32764 = No measurement data, 0..32000 |  |  |  |  | Process data value |
2 | 8 | 8-bit Integer |  |  |  |  |  | Process data scale | Scaling of the process data to calculate the measurement value: Process data x 10(scale) x [unit code] = measurement value Example: 327 x 10(-1) x [mm] = 32.7 mm
3 | 5 | 3-bit UInteger | 0 = 0: Low, 1 = 1: Low, 2 = 2: Low, 3 = 3: Low, 4 = 4: Sufficient, 5 = 5: Sufficient, 6 = 6: Good, 7 = 7: Good |  |  |  |  | Signal level | The signal level describes the strength of the received echo. The higher this numerical value, the stronger the echo.
4 | 2 | 3-bit UInteger | 0 = 0: Low, 1 = 1: Low, 2 = 2: Low, 3 = 3: Low, 4 = 4: Sufficient, 5 = 5: Sufficient, 6 = 6: Good, 7 = 7: Good |  |  |  |  | Signal stability (scaled) | Signal stability (scaled) is a simplified scaling of the index #1000/2 (Signal stability). It is determined cyclically by evaluating the echo signal. The higher this numerical value, the more stable the echo.
5 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Switch signal channel 1 state |
6 | 1 | Boolean | false = Inactive, true = Active |  |  |  |  | Signal channel 2 state |

Octet 0

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 1
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 1
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 2
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 3

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 3 | 4 | 6 | 5
element bit | 2 | 1 | 0 | 2 | 1 | 0 |  |

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 65 = SP1 single value teach-in, 66 = SP2 single value teach-in, 130 = Restore Factory Settings |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 65 = SP1 single value teach-in, 66 = SP2 single value teach-in, 130 = Restore Factory Settings
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  |  |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "microsonic GmbH"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "Unser Herz schallt ultra."
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
default value: "cube-340/FFIU"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
default value: "43440"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
default value: "Ultrasonic sensor"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Hardware Version" index=22 id=V_HardwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
default value: "***"
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Error Count" index=32 id=V_ErrorCount

data type: 16-bit UInteger
access rights: ro
dynamic

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure, 5..255 = Reserved
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

data type: Array[10] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48
subindex | 6 | 6 | 7 | 7 | 7 | 8 | 8 | 8

octet | 24 | 25 | 26 | 27 | 28 | 29 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 9 | 9 | 9 | 10 | 10 | 10 |

## Standard Variable "Process Data Input" index=40 id=V_ProcessDataInput

data type: see ProcessDataIn!
access rights: ro
dynamic
[Top]

## Variable "Function Tag" index=25 id=V_CP_FunctionTag

description: Possibility to mark a device with function-specific information.
data type: 32-octet String UTF-8
default value: "***"
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Location Tag" index=26 id=V_CP_LocationTag

description: Possibility to mark a device with location-specific information.
data type: 32-octet String UTF-8
default value: "***"
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Teach-in channel" index=58 id=V_SSP_TI_TeachSelect

description: Choice of channel for the next teach-in procedure
data type: 8-bit UInteger
allowed values: 1 = SSC1: pin 4 (push-pull), 2 = SSC2: pin 2 (push-pull), 192 = ASC1: pin 2 (current/volatge)
default value: 1
access rights: rw
excluded from data storage

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Teach-in Result" index=59 id=V_SSP_TI_TeachResult

data type: 8-bit Record (subindex access not supported)
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Idle, 1 = SP1 success, 2 = SP2 success, 3 = SP12 success, 4 = Wait for command, 5 = Busy, 7 = Error | 0 |  |  |  | Teach-in status |

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1
element bit |  |  |  |  | 3 | 2 | 1 | 0

## Variable "SSC1 parameter" index=60 id=V_SSP_SSC01_Param

data type: 64-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer | 350..5000 | 3400 |  |  |  | SP1 | Setpoint 1 for switching output
2 | 0 | 32-bit Integer | 350..5000 | 3900 |  |  |  | SP2 | Setpoint 2 for switching output

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "SSC1 configuration" index=61 id=V_SSP_SSC01_Config

data type: 48-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 40 | 8-bit UInteger | 0 = High active, 1 = Low active | 0 |  |  |  | Logic | Logic state for target detected
2 | 32 | 8-bit UInteger | 0 = Deactivated, 1 = Single point (SP1: switching point), 2 = Window (SP1, SP2: window mode), 3 = Two point (SP1, SP2: hysteresis mode), 128 = Single point + set point offset (SP1: switching point + offset), 129 = Window ± set point offset (SP1: two way reflective barrier) | 1 |  |  |  | Mode | Operation mode of the switch signal channel: switching point, window mode, hysteresis mode, switching point + offset, two way reflective barrier
3 | 0 | 32-bit Integer | 1..4650 | 50 |  |  |  | Hysteresis | Hysteresis for SP1 and SP2

octet | 0 | 1 | 2 | 3 | 4 | 5 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "SSC2 parameter" index=62 id=V_SSP_SSC02_Param

data type: 64-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer | 350..5000 | 1700 |  |  |  | SP1 | Setpoint 1 for switching output
2 | 0 | 32-bit Integer | 350..5000 | 2200 |  |  |  | SP2 | Setpoint 2 for switching output

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "SSC2 configuration" index=63 id=V_SSP_SSC02_Config

data type: 48-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 40 | 8-bit UInteger | 0 = High active, 1 = Low active | 0 |  |  |  | Logic | Logic state for target detected
2 | 32 | 8-bit UInteger | 0 = Deactivated, 1 = Single point (SP1: switching point), 2 = Window (SP1, SP2: window mode), 3 = Two point (SP1, SP2: hysteresis mode), 128 = Single point + set point offset (SP1: switching point + offset), 129 = Window ± set point offset (SP1: two way reflective barrier) | 1 |  |  |  | Mode | Operation mode of the switch signal channel: switching point, window mode, hysteresis mode, switching point + offset, two way reflective barrier
3 | 0 | 32-bit Integer | 1..4650 | 50 |  |  |  | Hysteresis | Hysteresis for SP1 and SP2

octet | 0 | 1 | 2 | 3 | 4 | 5 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "SSC1 advanced configuration" index=100 id=V_SSC01_AdvancedConfig

data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-on delay | Switch-on delay in seconds
2 | 8 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-off delay | Switch-off delay in seconds
3 | 0 | 8-bit UInteger | 2..20 | 8 |  |  |  | Set point offset | Offset value in % of SP1, which will be added to or subtracted from SP1.

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "SSC2 advanced configuration" index=101 id=V_SSC02_AdvancedConfig

data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-on delay | Switch-on delay in seconds
2 | 8 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-off delay | Switch-off delay in seconds
3 | 0 | 8-bit UInteger | 2..20 | 8 |  |  |  | Set point offset | Offset value in % of SP1, which will be added to or subtracted from SP1.

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "ASC1 parameter" index=160 id=V_ASC_Param

data type: 64-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer | 350..5000 | 350 |  |  |  | SP1 | Sensor-close or sensor-distant window margin (recommended sensor-close window margin)
2 | 0 | 32-bit Integer | 350..5000 | 3400 |  |  |  | SP2 | Sensor-distant or sensor-close window margin (recommended sensor-distant window margin)

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "ASC1 configuration" index=161 id=V_ASC_Config

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0 = Rising, 1 = Falling | 0 |  |  |  | Output characteristic | Rising or falling analogue characteristic
2 | 0 | 8-bit UInteger | 0 = disable ASC1 on pin 2 an activate SSC2 on pin 2, 1 = current output, 2 = voltage output, 3 = automatic detection on PowerUp | 3 |  |  |  | Operation mode | The operating mode of the ASC1 can be changed here.

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Measurement configuration" index=200 id=V_Messkonfig

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 16-bit UInteger | 350..1050 | 350 |  |  |  | Foreground suppression | The start of the measurement evaluation will be shifted from the blind zone to the value of the foreground suppression.

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 1 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Interference echo suppression" index=210 id=V_Stoerechoausblendung

description: With the function interference echo suppression, unwanted echoes in the application can be suppressed in up to three selected areas.
data type: 120-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 104 | 16-bit UInteger | 350..5000 | 2225 |  |  |  | Area 1 Start |
2 | 88 | 16-bit UInteger | 1..4650 | 200 |  |  |  | Area 1 Length |
3 | 80 | 8-bit UInteger | 0 = Deactivated, 1 = 10%, 2 = 20%, 3 = 30%, 4 = 40%, 5 = 50%, 6 = 60%, 7 = 70%, 8 = 80%, 9 = 90%, 10 = 100% | 0 |  |  |  | Area 1 Sensitivity damping |
4 | 64 | 16-bit UInteger | 350..5000 | 3400 |  |  |  | Area 2 Start |
5 | 48 | 16-bit UInteger | 1..4650 | 200 |  |  |  | Area 2 Length |
6 | 40 | 8-bit UInteger | 0 = Deactivated, 1 = 10%, 2 = 20%, 3 = 30%, 4 = 40%, 5 = 50%, 6 = 60%, 7 = 70%, 8 = 80%, 9 = 90%, 10 = 100% | 0 |  |  |  | Area 2 Sensitivity damping |
7 | 24 | 16-bit UInteger | 350..5000 | 4200 |  |  |  | Area 3 Start |
8 | 8 | 16-bit UInteger | 1..4650 | 200 |  |  |  | Area 3 Length |
9 | 0 | 8-bit UInteger | 0 = Deactivated, 1 = 10%, 2 = 20%, 3 = 30%, 4 = 40%, 5 = 50%, 6 = 60%, 7 = 70%, 8 = 80%, 9 = 90%, 10 = 100% | 0 |  |  |  | Area 3 Sensitivity damping |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56
subindex | 1 | 1 | 2 | 2 | 3 | 4 | 4 | 5
element bit | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 | 15 - 8

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 |
bit offset | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 5 | 6 | 7 | 7 | 8 | 8 | 9 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "Detection area width & sensitivity" index=220 id=V_Empfindlichkeit

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0 = Narrow & Low, 1 = Normal & Standard, 2 = Wide & High | 1 |  |  |  | Setting |
2 | 0 | 8-bit UInteger | 0 = Inaktiv, 1 = Aktiv | 0 |  |  |  | Sensitivity hysteresis | Sensitivity hysteresis at lateral object entry for a more stable detection behavior

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Filter" index=256 id=V_Filter

data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 8-bit UInteger | 0 = F00: no filter, 1 = F01: standard filter, 2 = F02: averaging filter | 1 |  |  |  | Type | Measurement filter for the evaluation of the measured values
2 | 8 | 8-bit UInteger | 0 = P00: weak filter, 1 = P01, 2 = P02, 3 = P03, 4 = P04, 5 = P05, 6 = P06, 7 = P07, 8 = P08, 9 = P09: strong filter | 0 |  |  |  | Strength | Strength of the chosen measurement filter
3 | 0 | 8-bit Integer | 10..25 | 25 |  |  |  | Maximum object speed | Maximum object speed for a movement towards and away from the sensor. Valid (only) for type F01 and F02.

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Temperature compensation" index=300 id=V_TempKomp

description: The sensor is equipped with an internal temperature unit in order to determine the ambient temperature and to compensate the temperature dependency of the sound velocity in air. Alternatively, a reference temperature can be set manually.
data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0 = Reference temperature, 1 = Assumed air temperature | 1 |  |  |  | Temperature source | Evaluate assumed air temperature or use reference temperature.
2 | 0 | 8-bit Integer | -25..70 | 20 |  |  |  | Reference temperature | Manually set reference temperature for the temperature compensation

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Synchronisation and multiplex operation" index=350 id=V_SyncMux

data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 8-bit UInteger | 0 = Inactive, 1 = Active | 1 |  |  |  | Mode |
2 | 8 | 8-bit UInteger | 0 = Synchronisation active, 1 = Multiplex address 1, 2 = Multiplex address 2, 3 = Multiplex address 3, 4 = Multiplex address 4, 5 = Multiplex address 5, 6 = Multiplex address 6, 7 = Multiplex address 7, 8 = Multiplex address 8, 9 = Multiplex address 9, 10 = Multiplex address 10, 128 = IO-Link synchronisation active | 0 |  |  |  | Sensor operation |
3 | 0 | 8-bit UInteger | 2 = 2 participants, 3 = 3 participants, 4 = 4 participants, 5 = 5 participants, 6 = 6 participants, 7 = 7 participants, 8 = 8 participants, 9 = 9 participants, 10 = 10 participants | 10 |  |  |  | Multiplex number of participants | Maximum number of multiplex participants should be adjusted to correct number of participants in order to speed up multiplex operation.

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Control" index=370 id=V_BedienungEingabe

data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Teach-in buttons and teach-in via pin 5 inactive, 1 = Teach-in buttons inactive and teach-in via pin 5 active, 2 = Teach-in buttons active and teach-in via pin 5 inactive, 3 = Teach-in buttons and teach-in via pin 5 active | 2 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "LED" index=371 id=V_BedienungAusgabe

data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Inactive, 1 = Active | 1 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Signal quality" index=1000 id=V_EchoDiagnose

data type: 24-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 16-bit UInteger |  | 0 |  |  |  | Amplitude |
2 | 0 | 8-bit UInteger |  | 0 |  |  |  | Signal stability | The signal stability is determined cyclically by evaluating the echo signal. The higher this numerical value, the more stable the echo. 0...31: Low, 32...47: Sufficient, 48...63: Good

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 2 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "Diagnosis of temperature compensation" index=2000 id=V_DiagnoseTemperatur

data type: 24-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 16-bit Integer |  | 0 |  |  |  | Assumed air temperature |
2 | 0 | 8-bit UInteger | 0 = Not completed, 1 = Completed | 0 |  |  |  | Heating-up phase |

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 2 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "Measurement data channel description" index=16512 id=V_SSP_MDC_Descriptor

data type: 88-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 56 | 32-bit Integer |  | 350 |  |  |  | Lower limit | Lower limit of the measuring range (blind zone)
2 | 24 | 32-bit Integer |  | 5000 |  |  |  | Upper limit | Upper limit of the measuring range (maximum range)
3 | 8 | 16-bit UInteger |  | 1013 |  |  |  | Unit code | IO-Link unit code: 1013 = [mm]
4 | 0 | 8-bit Integer |  | 0 |  |  |  | Scale | Process data value * (10 ^ scale) [Unit code] = measuring value in mm

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 4 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

[Top]

## ErrorTypes

Code | Additional code | Name | Description
--- | --- | --- | ---
129 (0x81) | 0 (0x00) | Parameter SP1 cannot be teached/set under VGA. |
129 (0x81) | 1 (0x01) | Parameter SP2 cannot be teached/set under VGA. |
129 (0x81) | 2 (0x02) | Parameter SP1 cannot be teached/set above GT. |
129 (0x81) | 3 (0x03) | Parameter SP2 cannot be teached/set above GT. |
129 (0x81) | 4 (0x04) | Parameter SP1 cannot be teached/set above GT - HY. |
129 (0x81) | 5 (0x05) | Parameter SP2 cannot be teached/set above GT - HY. |
129 (0x81) | 6 (0x06) | Parameter SP1 cannot be teached/set under VGA + HY. |
129 (0x81) | 7 (0x07) | Parameter SP2 cannot be teached/set under VGA + HY. |
129 (0x81) | 8 (0x08) | The distance between parameters SP1 and SP2 must be at least 2x hysteresis. |
129 (0x81) | 9 (0x09) | Parameter SP1 cannot be teached/set above GT - HY - Offset. |
129 (0x81) | 10 (0x0a) | Parameter SP1 cannot be teached/set under VGA + HY + Offset. |
129 (0x81) | 11 (0x0b) | The distance between parameters SP1 and SP2 must be at least 1 mm. |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
16384 (0x4000) | Error | Temperature fault | Overload
16912 (0x4210) | Warning | Device temperature over-run | Clear source of heat
16928 (0x4220) | Warning | Device temperature under-run | Insulate device
20736 (0x5100) | Error | General power supply fault | Check availability
30480 (0x7710) | Error | Short circuit | Check installation
36000 (0x8ca0) | Notification | Teach-in error | Teach-in process was not successful.
36001 (0x8ca1) | Notification | Teach-in success | Teach-in process was successful.
36002 (0x8ca2) | Notification | CycleTime error | CycleTime error is triggered if cycle time does not correspond to the permitted configuration.

[Top]

## Process Data Formatting

Formatting for Process Data id=PI_PDI32_MSDC32
Subindex 1: * 1 + 0 mm Dec.0
Subindex 2: * 1 + 0 Dec.0
Subindex 3: * 1 + 0 Dec.0
Subindex 4: * 1 + 0 Dec.0
Subindex 5:
Subindex 6:

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_HardwareRevision
V_FirmwareRevision
V_ApplicationSpecificTag, rw
V_CP_FunctionTag, rw
V_CP_LocationTag, rw

Observation Menu
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSP_SSC01_Param.SP1 * 1 + 0 mm, ro Dec.0
V_SSP_SSC01_Param.SP2 * 1 + 0 mm, ro Dec.0
V_SSP_SSC01_Config.Logic, ro
V_SSP_SSC01_Config.Mode, ro
V_SSP_SSC01_Config.Hysteresis * 1 + 0 mm, ro Dec.0
V_SSC01_AdvancedConfig.Switch-on delay * 0.1 + 0 s, ro Dec.1
V_SSC01_AdvancedConfig.Switch-off delay * 0.1 + 0 s, ro Dec.1
V_SSC01_AdvancedConfig.Set point offset * 1 + 0 %, ro Dec.0
SSC2: switch signal channel 2 - pin 2 (push-pull)
V_SSP_SSC02_Param.SP1 * 1 + 0 mm, ro Dec.0
V_SSP_SSC02_Param.SP2 * 1 + 0 mm, ro Dec.0
V_SSP_SSC02_Config.Logic, ro
V_SSP_SSC02_Config.Mode, ro
V_SSP_SSC02_Config.Hysteresis * 1 + 0 mm, ro Dec.0
V_SSC02_AdvancedConfig.Switch-on delay * 0.1 + 0 s, ro Dec.1
V_SSC02_AdvancedConfig.Switch-off delay * 0.1 + 0 s, ro Dec.1
V_SSC02_AdvancedConfig.Set point offset * 1 + 0 %, ro Dec.0
ASC1: analogue signal channel 1 - pin 2 (current/voltage)
V_ASC_Param.SP1 * 1 + 0 mm, ro Dec.0
V_ASC_Param.SP2 * 1 + 0 mm, ro Dec.0
V_ASC_Config.Output characteristic, ro
V_ASC_Config.Operation mode, ro
Filter
V_Filter.Type, ro
V_Filter.Strength, ro
V_Filter.Maximum object speed * 0.1 + 0 m/s, ro Dec.1
Temperature compensation
V_TempKomp.Temperature source, ro
V_TempKomp.Reference temperature * 1 + 0 °C, ro Dec.0
Detection area width & sensitivity
V_Empfindlichkeit.Setting, rw
V_Empfindlichkeit.Sensitivity hysteresis, rw
Interference echo suppression
V_Messkonfig.Foreground suppression * 1 + 0 mm, ro Dec.0
V_Stoerechoausblendung.Area 1 Start * 1 + 0 mm, ro Dec.0
V_Stoerechoausblendung.Area 1 Length * 1 + 0 mm, ro Dec.0
V_Stoerechoausblendung.Area 1 Sensitivity damping, ro
V_Stoerechoausblendung.Area 2 Start * 1 + 0 mm, ro Dec.0
V_Stoerechoausblendung.Area 2 Length * 1 + 0 mm, ro Dec.0
V_Stoerechoausblendung.Area 2 Sensitivity damping, ro
V_Stoerechoausblendung.Area 3 Start * 1 + 0 mm, ro Dec.0
V_Stoerechoausblendung.Area 3 Length * 1 + 0 mm, ro Dec.0
V_Stoerechoausblendung.Area 3 Sensitivity damping, ro
Synchronisation and multiplex operation
V_SyncMux.Mode, ro
V_SyncMux.Sensor operation, ro
V_SyncMux.Multiplex number of participants, ro
User interface
V_BedienungEingabe.Mode, ro
V_BedienungAusgabe.Mode, ro
Diagnosis of temperature compensation
V_DiagnoseTemperatur.Assumed air temperature * 0.1 + 0 °C, ro Dec.1
V_DiagnoseTemperatur.Heating-up phase, ro
Signal quality
V_EchoDiagnose.Amplitude, ro
V_EchoDiagnose.Signal stability, ro
ProcessDataInput
V_ProcessDataInput.1 * 1 + 0 mm, ro Dec.0
V_ProcessDataInput.2 * 1 + 0, ro Dec.0
V_ProcessDataInput.3 * 1 + 0, ro Dec.0
V_ProcessDataInput.4 * 1 + 0, ro Dec.0
V_ProcessDataInput.5, ro
V_ProcessDataInput.6, ro

Diagnosis Menu
Device status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus
Measurement data channel description
V_SSP_MDC_Descriptor.Lower limit * 1 + 0 mm, ro Dec.0
V_SSP_MDC_Descriptor.Upper limit * 1 + 0 mm, ro Dec.0
V_SSP_MDC_Descriptor.Unit code, ro
V_SSP_MDC_Descriptor.Scale, ro

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_HardwareRevision
V_FirmwareRevision
V_ApplicationSpecificTag, rw
V_CP_FunctionTag, rw
V_CP_LocationTag, rw

Parameter Menu
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSP_SSC01_Param.SP1 * 1 + 0 mm, rw Dec.0
V_SSP_SSC01_Param.SP2 * 1 + 0 mm, rw Dec.0
V_SSP_SSC01_Config.Logic, rw
V_SSP_SSC01_Config.Mode, rw
V_SSP_SSC01_Config.Hysteresis * 1 + 0 mm, rw Dec.0
V_SSC01_AdvancedConfig.Switch-on delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Switch-off delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Set point offset * 1 + 0 %, rw Dec.0
SSC2: switch signal channel 2 - pin 2 (push-pull)
V_SSP_SSC02_Param.SP1 * 1 + 0 mm, rw Dec.0
V_SSP_SSC02_Param.SP2 * 1 + 0 mm, rw Dec.0
V_SSP_SSC02_Config.Logic, rw
V_SSP_SSC02_Config.Mode, rw
V_SSP_SSC02_Config.Hysteresis * 1 + 0 mm, rw Dec.0
V_SSC02_AdvancedConfig.Switch-on delay * 0.1 + 0 s, rw Dec.1
V_SSC02_AdvancedConfig.Switch-off delay * 0.1 + 0 s, rw Dec.1
V_SSC02_AdvancedConfig.Set point offset * 1 + 0 %, rw Dec.0
ASC1: analogue signal channel 1 - pin 2 (current/voltage)
V_ASC_Param.SP1 * 1 + 0 mm, rw Dec.0
V_ASC_Param.SP2 * 1 + 0 mm, rw Dec.0
V_ASC_Config.Output characteristic, rw
V_ASC_Config.Operation mode, rw
Teach-in channel
V_SSP_TI_TeachSelect
V_SystemCommand, Button:=65
V_SystemCommand, Button:=66
V_SSP_TI_TeachResult
Filter
V_Filter.Type, rw
V_Filter.Strength, rw
V_Filter.Maximum object speed * 0.1 + 0 m/s, rw Dec.1
Temperature compensation
V_TempKomp.Temperature source, rw
V_TempKomp.Reference temperature * 1 + 0 °C, rw Dec.0
Detection area width & sensitivity
V_Empfindlichkeit.Setting, rw
V_Empfindlichkeit.Sensitivity hysteresis, rw
Interference echo suppression
V_Messkonfig.Foreground suppression * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 1 Start * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 1 Length * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 1 Sensitivity damping, rw
V_Stoerechoausblendung.Area 2 Start * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 2 Length * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 2 Sensitivity damping, rw
V_Stoerechoausblendung.Area 3 Start * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 3 Length * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 3 Sensitivity damping, rw
Synchronisation and multiplex operation
V_SyncMux.Mode, rw
V_SyncMux.Sensor operation, rw
V_SyncMux.Multiplex number of participants, rw
User interface
V_BedienungEingabe.Mode, rw
V_BedienungAusgabe.Mode, rw
System command
V_SystemCommand, Button:=130
Device access locks
V_DeviceAccessLocks.Parameter (write) Access Lock, rw
V_DeviceAccessLocks.Local Parameterization Lock, rw

Observation Menu
Diagnosis of temperature compensation
V_DiagnoseTemperatur.Assumed air temperature * 0.1 + 0 °C, ro Dec.1
V_DiagnoseTemperatur.Heating-up phase, ro
Signal quality
V_EchoDiagnose.Amplitude, ro
V_EchoDiagnose.Signal stability, ro
ProcessDataInput
V_ProcessDataInput.1 * 1 + 0 mm, ro Dec.0
V_ProcessDataInput.2 * 1 + 0, ro Dec.0
V_ProcessDataInput.3 * 1 + 0, ro Dec.0
V_ProcessDataInput.4 * 1 + 0, ro Dec.0
V_ProcessDataInput.5, ro
V_ProcessDataInput.6, ro

Diagnosis Menu
Device status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus
Measurement data channel description
V_SSP_MDC_Descriptor.Lower limit * 1 + 0 mm, ro Dec.0
V_SSP_MDC_Descriptor.Upper limit * 1 + 0 mm, ro Dec.0
V_SSP_MDC_Descriptor.Unit code, ro
V_SSP_MDC_Descriptor.Scale, ro

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_HardwareRevision
V_FirmwareRevision
V_ApplicationSpecificTag, rw
V_CP_FunctionTag, rw
V_CP_LocationTag, rw

Parameter Menu
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSP_SSC01_Param.SP1 * 1 + 0 mm, rw Dec.0
V_SSP_SSC01_Param.SP2 * 1 + 0 mm, rw Dec.0
V_SSP_SSC01_Config.Logic, rw
V_SSP_SSC01_Config.Mode, rw
V_SSP_SSC01_Config.Hysteresis * 1 + 0 mm, rw Dec.0
V_SSC01_AdvancedConfig.Switch-on delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Switch-off delay * 0.1 + 0 s, rw Dec.1
V_SSC01_AdvancedConfig.Set point offset * 1 + 0 %, rw Dec.0
SSC2: switch signal channel 2 - pin 2 (push-pull)
V_SSP_SSC02_Param.SP1 * 1 + 0 mm, rw Dec.0
V_SSP_SSC02_Param.SP2 * 1 + 0 mm, rw Dec.0
V_SSP_SSC02_Config.Logic, rw
V_SSP_SSC02_Config.Mode, rw
V_SSP_SSC02_Config.Hysteresis * 1 + 0 mm, rw Dec.0
V_SSC02_AdvancedConfig.Switch-on delay * 0.1 + 0 s, rw Dec.1
V_SSC02_AdvancedConfig.Switch-off delay * 0.1 + 0 s, rw Dec.1
V_SSC02_AdvancedConfig.Set point offset * 1 + 0 %, rw Dec.0
ASC1: analogue signal channel 1 - pin 2 (current/voltage)
V_ASC_Param.SP1 * 1 + 0 mm, rw Dec.0
V_ASC_Param.SP2 * 1 + 0 mm, rw Dec.0
V_ASC_Config.Output characteristic, rw
V_ASC_Config.Operation mode, rw
Teach-in channel
V_SSP_TI_TeachSelect
V_SystemCommand, Button:=65
V_SystemCommand, Button:=66
V_SSP_TI_TeachResult
Filter
V_Filter.Type, rw
V_Filter.Strength, rw
V_Filter.Maximum object speed * 0.1 + 0 m/s, rw Dec.1
Temperature compensation
V_TempKomp.Temperature source, rw
V_TempKomp.Reference temperature * 1 + 0 °C, rw Dec.0
Detection area width & sensitivity
V_Empfindlichkeit.Setting, rw
V_Empfindlichkeit.Sensitivity hysteresis, rw
Interference echo suppression
V_Messkonfig.Foreground suppression * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 1 Start * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 1 Length * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 1 Sensitivity damping, rw
V_Stoerechoausblendung.Area 2 Start * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 2 Length * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 2 Sensitivity damping, rw
V_Stoerechoausblendung.Area 3 Start * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 3 Length * 1 + 0 mm, rw Dec.0
V_Stoerechoausblendung.Area 3 Sensitivity damping, rw
Synchronisation and multiplex operation
V_SyncMux.Mode, rw
V_SyncMux.Sensor operation, rw
V_SyncMux.Multiplex number of participants, rw
User interface
V_BedienungEingabe.Mode, rw
V_BedienungAusgabe.Mode, rw
System command
V_SystemCommand, Button:=130
Device access locks
V_DeviceAccessLocks.Parameter (write) Access Lock, rw
V_DeviceAccessLocks.Local Parameterization Lock, rw

Observation Menu
Diagnosis of temperature compensation
V_DiagnoseTemperatur.Assumed air temperature * 0.1 + 0 °C, ro Dec.1
V_DiagnoseTemperatur.Heating-up phase, ro
Signal quality
V_EchoDiagnose.Amplitude, ro
V_EchoDiagnose.Signal stability, ro
ProcessDataInput
V_ProcessDataInput.1 * 1 + 0 mm, ro Dec.0
V_ProcessDataInput.2 * 1 + 0, ro Dec.0
V_ProcessDataInput.3 * 1 + 0, ro Dec.0
V_ProcessDataInput.4 * 1 + 0, ro Dec.0
V_ProcessDataInput.5, ro
V_ProcessDataInput.6, ro

Diagnosis Menu
Device status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus
Measurement data channel description
V_SSP_MDC_Descriptor.Lower limit * 1 + 0 mm, ro Dec.0
V_SSP_MDC_Descriptor.Upper limit * 1 + 0 mm, ro Dec.0
V_SSP_MDC_Descriptor.Unit code, ro
V_SSP_MDC_Descriptor.Scale, ro

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.