Version: V131504.691436 | Release Date: 2020-10-02

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Menus]

bks+3/FIU
Vendor ID | 419 (0x01a3) |
Vendor Name | microsonic GmbH
Vendor Text | Unser Herz schallt ultra.
Vendor URL | http://www.microsonic.de
Device ID | 23 (0x000017)
DeviceFamily | bks+
Features
Block Parameter | yes
Data Storage | yes
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: no, Local User Interface: no
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 4 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_1_2 with 2 octets on-request data OPERATE = TYPE_2_2 with 1 octet on-request data ISDU supported
Device Variant | bks+3/FIU
--- | ---
Description | Ultrasound web edge sensor with 1 push-pull switching output, 100 mA load capacity, analogue current or voltage output, 4..20 mA or 0..10 V, detection range 12 mm, IODD valid for: bks+3/FIU
Product ID | bks+3/FIU
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC
Device Variant | bks+3/FIU/001
Description | Ultrasound web edge sensor with 1 push-pull switching output, 100 mA load capacity, analogue current or voltage output, 4..20 mA or 0..10 V, detection range 12 mm, IODD valid for: bks+3/FIU/001
Product ID | bks+3/FIU/001
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "Measured value" id=PD_ProcessDataIn

bit length: 16
data type: 16-bit Record

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 16-bit UInteger |  |  |  |  |  | Measured value |

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 1 |
element bit | 15 - 8 | 7 - 0 |

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 130 = Restore Factory Settings, 161 = Sensor adjustment: fork cleared , 162 = Sensor adjustment: fork 50 % covered , 163 = Sensor adjustment: fork 100 % covered , 164 = Reset to factory setting |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 130 = Restore Factory Settings, 161 = Sensor adjustment: fork cleared , 162 = Sensor adjustment: fork 50 % covered , 163 = Sensor adjustment: fork 100 % covered , 164 = Reset to factory setting
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  |  |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "microsonic GmbH"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "www.microsonic.de"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
default value: "bks+"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
default value: "bks+3/FIU "
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
default value: "Ultraschall-Sensor"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Hardware Version" index=22 id=V_HardwareRevision

data type: 64-octet String UTF-8
default value: "-"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
default value: "-"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

[Top]

## Variable "Teach-in via push-button" index=64 id=V_pushbutton

description: The push-button can be activated/deactivated for sensor settings with Teach-in.
data type: 8-bit UInteger
allowed values: 0 = enabled, 1 = disable
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Linearisation of the output characteristic" index=65 id=V_linearisation

description: To increase the absolute accuracy in the edge areas, the linearisation of the output characteristic can be disabled.
data type: 8-bit UInteger
allowed values: 0 = disable, 1 = enabled
default value: 1
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Temperature compensation" index=66 id=V_temp_compensation

description: The temperature compensation is used for measument value correction for varying ambient temperatures and can be disabled.
data type: 8-bit UInteger
allowed values: 0 = disable, 1 = enabled
default value: 1
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Analogue output mode" index=68 id=V_analogue_output_mode

description: For the analog output either the function output voltage or current output can be selected.
data type: 8-bit UInteger
allowed values: 2 = Analogue current output, 3 = Analogue voltage output
default value: 3
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Rising / falling analogue characteristic" index=69 id=V_analogue_output_polarity

description: The analogue characteristic can be set on rising (0 V / 4 mA at full coverage) or falling characteristic.
data type: 8-bit UInteger
allowed values: 0 = Rising characteristic curve, 1 = Falling characteristic curve
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Set NOC/NCC" index=70 id=V_switched_output_polarity

description: The NCC or NOC output function can be present for the switched output.
data type: 8-bit UInteger
allowed values: 0 = NOC, 1 = NCC
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "LED deactivation" index=72 id=V_led

description: When activated, the LEDs are switched off 30 seconds after a key press. After a new key press they will run for 30 seconds.
data type: 8-bit UInteger
allowed values: 0 = disable, 1 = enabled
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Measurement filter" index=77 id=V_filter_type

description: bks+ ultrasonic sensors provide for a choice of 3 filter settings: F00: no filter | F01: average value filter | F02: median filter
data type: 8-bit UInteger
allowed values: 0 = F00, 1 = F01, 2 = F02
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Filter strength" index=78 id=V_filter_strength

description: For each measurement value filter, a filter strength between 0 (weak filter effect) and 9 (strong filter effect) can be selected.
data type: 8-bit UInteger
allowed values: 0 = P00, 1 = P01, 2 = P02, 3 = P03, 4 = P04, 5 = P05, 6 = P06, 7 = P07, 8 = P08, 9 = P09
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Center of switching window" index=79 id=V_switched_output_position

description: If the web edge is within the switching window the switching output is set. The switching window is defined by the adjusted center and the width.
data type: 16-bit Integer
allowed values: 0..4095
default value: 2047
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "width of switching window" index=80 id=V_switched_output_width

description: If the web edge is within the switching window the switching output is set. The switching window is defined by the adjusted center and the width.
data type: 16-bit UInteger
allowed values: 0..4095
default value: 1023
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Process data" index=84 id=V_process_data

description: This field shows the measured value at the time of reading.
data type: 16-bit UInteger
allowed values: 0..4095
default value: 0
access rights: ro

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
36000 (0x8ca0) | Notification | Parameter was changed | The parameter set of the sensor has been changed.
36001 (0x8ca1) | Notification | Sensor adjustment successfull | The adjustment has been completed successfully.
36002 (0x8ca2) | Notification | sensor adjustment failed | The sensor could not be adjusted.

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText

Observation Menu
V_analogue_output_mode * 1 + 0, ro
V_analogue_output_polarity * 1 + 0, ro
V_switched_output_polarity * 1 + 0, ro
V_switched_output_position * 0.002930403 + -6 mm, ro
V_switched_output_width * 0.002930403 + 0 mm, ro
V_filter_type * 1 + 0, ro
V_filter_strength * 1 + 0, ro
V_process_data * 1 + 0, ro

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText

Parameter Menu
V_filter_type * 1 + 0, rw
V_filter_strength * 1 + 0, rw
V_switched_output_position * 0.002930403 + -6 mm, rw
V_switched_output_width * 0.002930403 + 0 mm, rw
V_linearisation * 1 + 0, rw
V_temp_compensation * 1 + 0, rw
V_analogue_output_mode * 1 + 0, rw
V_analogue_output_polarity * 1 + 0, rw
V_switched_output_polarity * 1 + 0, rw
V_pushbutton * 1 + 0, rw
V_led * 1 + 0, rw
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164

Observation Menu
V_process_data * 1 + 0, ro

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_HardwareRevision
V_FirmwareRevision

Parameter Menu
V_process_data * 1 + 0, ro
V_filter_type * 1 + 0, rw
V_filter_strength * 1 + 0, rw
V_switched_output_position * 0.002930403 + -6 mm, rw
V_switched_output_width * 0.002930403 + 0 mm, rw
V_linearisation * 1 + 0, rw
V_temp_compensation * 1 + 0, rw
V_analogue_output_mode * 1 + 0, rw
V_analogue_output_polarity * 1 + 0, rw
V_switched_output_polarity * 1 + 0, rw
V_pushbutton * 1 + 0, rw
V_led * 1 + 0, rw
V_SystemCommand, Button:=130
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
V_DeviceAccessLocks, rw

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.