Version: V164653.514512 | Release Date: 2016-10-26

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Menus]

sks-15/CF
Vendor ID | 419 (0x01a3) |
Vendor Name | microsonic GmbH
Vendor Text | Unser Herz schallt ultra.
Vendor URL | http://www.microsonic.de
Device ID | 27 (0x00001b)
DeviceFamily | sks
Features
Block Parameter | yes
Data Storage | yes
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: no
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 8 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_1_2 with 2 octets on-request data OPERATE = TYPE_2_2 with 1 octet on-request data ISDU supported
Device Variant | sks-15/CF
--- | ---
Description | Ultrasonic proximity switch with 1 push-pull switched output, loadable to 100 mA, 150 mm operating range.
Product ID | sks-15/CF
Device Icon |
Device Symbol |
Connection Type | M8 connector
Connection Symbol |
- pin 1 | brown; L+
- pin 2 | white; NC
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "The measured distance value is output with a resolution of 0,1 mm." id=PD_ProcessDataIn

bit length: 16
data type: 16-bit Record

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 1 | 15-bit UInteger |  |  |  |  |  | Prozess Data |
2 | 0 | Boolean | false = Not connected, true = Connected |  |  |  |  | Switching status |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 1
element bit | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 1 | 2
element bit | 6 | 5 | 4 | 3 | 2 | 1 | 0 |

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 130 = Restore Factory Settings, 161 = Teach one detect point, 162 = Teach one detect point 8% behind object, 164 = Window-Mode: Teach two-way barrier, 165 = Window-Mode: Teach first detect point, 166 = Window-Mode: Teach second detect point |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 130 = Restore Factory Settings, 161 = Teach one detect point, 162 = Teach one detect point 8% behind object, 164 = Window-Mode: Teach two-way barrier, 165 = Window-Mode: Teach first detect point, 166 = Window-Mode: Teach second detect point
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  |  |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "microsonic GmbH"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "Unser Herz schallt ultra."
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
default value: "sks-15/CF"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
default value: "sks-15/CF"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
default value: "Ultraschall-Sensor"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
default value: "********************************"
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

[Top]

## Variable "Switching point 1 (SP1)" index=64 id=V_S1_Schaltpunkt1

description: Switched output is reactivated when distance to an object is greater than RP1 (SP1 + hysteresis). Adjusting range: 20…249 mm Pointer: RP1 must be greater than SP1.
data type: 16-bit UInteger
allowed values: 356..4452
default value: 2671
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Return switching point 1 (RP1)" index=65 id=V_S1_Rueckschaltpunkt1

description: Switched output is reactivated when distance to an object is greater than RP1 (SP1 + hysteresis). Adjusting range: 21…250 mm Pointer: RP1 must be greater than SP1.
data type: 16-bit UInteger
allowed values: 356..4452
default value: 2707
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "NO/NC operation" index=66 id=V_S1_Logik

description: The NC or NO output function can be preset for the switched output.
data type: 8-bit UInteger
allowed values: 0 = NO normally open, 1 = NC normally closed
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Filter" index=67 id=V_FilterTyp

description: There are 5 filter settings: F00: No filter | F01: standard filter | F02: average value filter | F03: foreground filter | F04: background filter
data type: 8-bit UInteger
allowed values: 0 = F00, 1 = F01, 2 = F02, 3 = F03, 4 = F04
default value: 1
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Filter strength" index=68 id=V_FilterStaerke

description: A filter strength between 0 – weak filter effect – and 9 – pronounced filter effect – can be selected for each measurement filter.
data type: 8-bit UInteger
allowed values: 0 = P00, 1 = P01, 2 = P02, 3 = P03, 4 = P04, 5 = P05, 6 = P06, 7 = P07, 8 = P08, 9 = P09
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Switching point 2 (SP2)" index=71 id=V_S1_Rueckschaltpunkt2

description: Switched output is activated when distance to an object is shorter than SP2. Adjusting range: 22…3000 mm Pointer: SP2 must be greater than RP1. If SP2 or RP2 are greater than 250 mm, window mode is disabled.
data type: 16-bit UInteger
allowed values: 356..53426
default value: 53426
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Return switching point 2 (RP2)" index=72 id=V_S1_Schaltpunkt2

description: Switched output is reactivated when distance to an object is greater than RP2. Adjusting range: 23…3000 mm Pointer: RP2 must be greater than SP2. If SP2 or RP2 are greater than 250 mm, window mode is disabled.
data type: 16-bit UInteger
allowed values: 356..53426
default value: 53426
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Teach-In via button" index=74 id=V_TeachIn_per_Taste

description: Activate/Deactivate external teach in via Button.
data type: 8-bit UInteger
allowed values: 0 = enable, 1 = disable
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Detection range" index=75 id=V_Tastweite

description: Maximum detection range of the sensor. Adjusting range: 300…500 mm
data type: 16-bit UInteger
allowed values: 5343..8904
default value: 5343
access rights: rw

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Temperature Compensation" index=76 id=V_TK_Modus

description: The temperature compensation may be activated or deactivated
data type: 8-bit UInteger
allowed values: 0 = disable, 1 = enable
default value: 0
access rights: rw

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
36000 (0x8ca0) | Notification | Teach-in fault | The last Teach-in operation has been canceled or terminated by an error. The determined settings are discarded.
36001 (0x8ca1) | Notification | Teach-in successful | The last Teach-in operation completed successfully. The determined settings are applied.
36002 (0x8ca2) | Notification | MasterCycleTime is invalid | The CycleTime choosen by the Master exceeds or falls below the limits of the device. Range: 8 ms … 134,3 ms

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_ApplicationSpecificTag

Observation Menu
Measurement configuration
V_Tastweite * 0.05615234 + 0 mm, ro
Switching output
Configuration
V_S1_Logik, ro
Parameter
V_S1_Schaltpunkt1 * 0.05615234 + 0 mm, ro
V_S1_Rueckschaltpunkt1 * 0.05615234 + 0 mm, ro
V_S1_Rueckschaltpunkt2 * 0.05615234 + 0 mm, ro
V_S1_Schaltpunkt2 * 0.05615234 + 0 mm, ro
Filter
V_FilterTyp, ro
V_FilterStaerke, ro

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_ApplicationSpecificTag

Observation Menu
Measurement configuration
V_Tastweite * 0.05615234 + 0 mm, ro
Switching output
Configuration
V_S1_Logik, rw
Parameter
V_S1_Schaltpunkt1 * 0.05615234 + 0 mm, rw
V_S1_Rueckschaltpunkt1 * 0.05615234 + 0 mm, rw
V_S1_Rueckschaltpunkt2 * 0.05615234 + 0 mm, rw
V_S1_Schaltpunkt2 * 0.05615234 + 0 mm, rw
Filter
V_FilterTyp, ro
V_FilterStaerke, ro
Standard Command
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162
V_SystemCommand, Button:=165
V_SystemCommand, Button:=166
V_SystemCommand, Button:=164

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_FirmwareRevision
V_ApplicationSpecificTag, rw

Parameter Menu
Measurement configuration
V_Tastweite * 0.05615234 + 0 mm, rw
Switching output
Configuration
V_S1_Logik, rw
Parameter
V_S1_Schaltpunkt1 * 0.05615234 + 0 mm, rw
V_S1_Rueckschaltpunkt1 * 0.05615234 + 0 mm, rw
V_S1_Rueckschaltpunkt2 * 0.05615234 + 0 mm, rw
V_S1_Schaltpunkt2 * 0.05615234 + 0 mm, rw
Filter
V_FilterTyp, rw
V_FilterStaerke, rw
Temperature Compensation
V_TK_Modus, rw
Controls
V_TeachIn_per_Taste, rw
Standard Command
V_SystemCommand, Button:=130
V_SystemCommand, Button:=161
V_SystemCommand, Button:=162
V_SystemCommand, Button:=165
V_SystemCommand, Button:=166
V_SystemCommand, Button:=164
DeviceAccessLocks
V_DeviceAccessLocks.Parameter (write) Access Lock, rw
V_DeviceAccessLocks.Data Storage Lock, rw
V_DeviceAccessLocks.Local Parameterization Lock, rw

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.