Version: V175908.366942 | Release Date: 2019-07-02

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Process Data Formatting]
[Menus]

esf-1/CDF/A
Vendor ID | 419 (0x01a3) |
Vendor Name | microsonic GmbH
Vendor Text | Unser Herz schallt ultra.
Vendor URL | https://www.microsonic.de
Device ID | 72 (0x000048)
DeviceFamily | esf
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x0001 (Device Profile: Smart Sensor), 0x000a (Device Profile: ?Unknown?), 0x8000 (Function Class: Device Identification), 0x8003 (Function Class: Device Diagnosis), 0x800a (Function Class: ?Unknown?)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: yes
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 4 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_1_2 with 2 octets on-request data OPERATE = TYPE_2_V with 2 octets on-request data ISDU supported
Device Variant | esf-1/CDF/A
--- | ---
Description | Ultrasonic label and splice sensor, housing in fork format with fork depth 55 mm, 1 Push-Pull switching output, 1 pnp switching output, temperature compensation.
Product ID | 16950
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
Connection Symbol |
- pin 1 | brown; L+
- pin 2 | white; Other; pnp
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC; Com
Device Variant | esf-1/15/CDF/A
Description | Ultrasonic label and splice sensor, housing in fork format with fork depth 150 mm, 1 Push-Pull switching output, 1 pnp switching output, temperature compensation.
Product ID | 16952
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
Connection Symbol |
- pin 1 | brown; L+
- pin 2 | white; Other; pnp
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC; Com
Device Variant | esf-1/7/CDF/A
Description | Ultrasonic label and splice sensor, housing in fork format with fork depth 70 mm, 1 Push-Pull switching output, 1 pnp switching output, temperature compensation.
Product ID | 16953
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
Connection Symbol |
- pin 1 | brown; L+
- pin 2 | white; Other; pnp
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC; Com

[Top]

## ProcessData id=P_ProcessData

## ProcessDataIn "Process data" id=PI_ProcessDataIn

bit length: 32
data type: 32-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 16-bit Integer | -32760 = Out of measuring range (-), 32760 = Out of measuring range (+), 32764 = No measurement data, 0..1023 |  |  |  |  | Process data value |
2 | 8 | 8-bit Integer |  |  |  |  |  | Process data scale |
3 | 2 | Boolean | false = False, true = True |  |  |  |  | Web break |
4 | 1 | Boolean | false = False, true = True |  |  |  |  | Switch signal channel 2 state |
5 | 0 | Boolean | false = False, true = True |  |  |  |  | Switch signal channel 1 state |

Octet 0

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 1
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 1
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 2
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 3

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 3 | 4 | 5

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 75 = Teach-in start, 76 = Teach-in next step / end, 79 = Teach-in cancel, 130 = Restore Factory Settings |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 75 = Teach-in start, 76 = Teach-in next step / end, 79 = Teach-in cancel, 130 = Restore Factory Settings
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  |  |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "microsonic GmbH"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "Unser Herz schallt ultra."
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
default value: "Ultrasonic sensor"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Error Count" index=32 id=V_ErrorCount

data type: 16-bit UInteger
access rights: ro
dynamic

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
element bit | 15 - 8 | 7 - 0 |

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure, 5..255 = Reserved
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

data type: Array[10] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48
subindex | 6 | 6 | 7 | 7 | 7 | 8 | 8 | 8

octet | 24 | 25 | 26 | 27 | 28 | 29 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 9 | 9 | 9 | 10 | 10 | 10 |

## Standard Variable "Process Data Input" index=40 id=V_ProcessDataInput

data type: see ProcessDataIn!
access rights: ro
dynamic
[Top]

## Variable "Teach-in channel" index=58 id=V_TeachInChannel

description: Choice of channel for the next teach-in procedure
data type: 8-bit UInteger
allowed values: 0 = SSC1: Default: pin 4 (Push-Pull), 1 = SSC1: pin 4 (Push-Pull)
default value: 0
access rights: rw
excluded from data storage

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "Teach-in status" index=59 id=V_TeachInStatus

data type: 8-bit Record (subindex access not supported)
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Idle, 1 = SP1 success, 2 = SP2 success, 3 = SP12 success, 4 = Wait for command, 5 = Busy, 7 = Error | 0 |  |  |  | Status |

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1
element bit |  |  |  |  | 3 | 2 | 1 | 0

## Variable "SSC1 parameter" index=60 id=V_SSC1Param

data type: 32-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 16-bit Integer | 0..1023 | 300 |  |  |  | SP1 | Setpoint 1 for switch signal channel
2 | 0 | 16-bit Integer | 0..1023 | 508 |  |  |  | SP2 | Setpoint 2 for switch signal channel

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 2 | 2 |
element bit | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "SSC1 configuration" index=61 id=V_SSC1Config

data type: 32-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 8-bit UInteger | 0 = High active, 1 = Low active | 0 |  |  |  | Logic | Logical state of the switching signal channel
2 | 16 | 8-bit UInteger | 0 = Output deactivated, 1 = Only low threshold (SP1) (label/splice), 2 = Both thresholds (SP1 and SP2) (splice), 130 = Only high threshold (SP2) (splice) | 1 |  |  |  | Mode | Operation mode of the switch signal channel
3 | 0 | 16-bit Integer | 0..1023 | 8 | ro |  |  | Hysteresis | Hysteresis for SP1 and SP2

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "SSC2 parameter" index=62 id=V_SSC2Param

data type: 32-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 16-bit Integer | 0..1023 | 300 |  |  |  | SP1 | Setpoint 1 for switch signal channel
2 | 0 | 16-bit Integer | 0..1023 | 508 |  |  |  | SP2 | Setpoint 2 for switch signal channel

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 2 | 2 |
element bit | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "SSC2 configuration" index=63 id=V_SSC2Config

data type: 32-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 8-bit UInteger | 0 = Normally open, 1 = Normally closed | 0 |  |  |  | Logic | Logical state of the switching signal channel
2 | 16 | 8-bit UInteger | 0 = Output deactivated, 1 = Only low threshold (SP1) (label/splice), 2 = Both thresholds (SP1 and SP2) (splice), 130 = Only high threshold (SP2) (splice), 132 = Web break, 134 = Missing label, 135 = Mismatched label length | 132 |  |  |  | Mode | Operation mode of the switch signal channel
3 | 0 | 16-bit Integer | 0..1023 | 8 | ro |  |  | Hysteresis | Hysteresis for SP1 and SP2

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "SSC1 advanced configuration" index=100 id=V_SSC1AdvancedConfig

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-on delay | Switch-on delay in cycletimes
2 | 0 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-off delay | Switch-off delay in cycletimes

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "SSC2 advanced configuration" index=101 id=V_SSC2AdvancedConfig

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-on delay | Switch-on delay in cycletimes
2 | 0 | 8-bit UInteger | 0..255 | 0 |  |  |  | Switch-off delay | Switch-off delay in cycletimes

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Temperature compensation" index=300 id=V_TempKomp

description: The sensor is equipped with an internal temperature unit in order to determine the ambient temperature. Thus the temperature dependency of the loss of amplitude in air is compensated.
data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = off, 1 = on | 1 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Synchronisation" index=350 id=V_SyncMux

data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = off, 1 = on | 0 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Button and pin 5" index=370 id=V_BedienungEingabe

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 0 = Inactive, 1 = Button and pin 5 active, 2 = Only pin 5 active, 3 = Only button active | 1 |  |  |  | Teach-in input |
2 | 0 | 8-bit UInteger | 0 = Standard Teach-in methods, 1 = QuickTeach label sensor, 2 = QuickTeach splice sensor | 0 |  |  |  | Manual Teach-in method | With QuickTeach, you have a simplified Teach-in process that you have to activate once before initial commissioning.

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "LED" index=371 id=V_BedienungAusgabe

data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Inactive, 1 = Active, 4 = Find me! | 1 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Teach-in Feedback" index=372 id=V_BedienungFeedback

data type: 8-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Inactive, 1 = Feedback on pin 2 and pin 4, 2 = Feedback on pin 2, 3 = Feedback on pin 4 | 0 |  |  |  | Mode |

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Teach-in configuration" index=400 id=V_TeachInKonfig

data type: 16-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | 8-bit UInteger | 5..50 | 20 |  |  |  | Splice threshold | The splice threshold indicates the value by which the amplitude of the web material may vary in order to be evaluated as a splice.
2 | 0 | 8-bit UInteger | 0 = Label dynamic, 1 = Label static, 2 = Splice | 0 |  |  |  | Teach-in type | Label dynamic = Learn both backing material and label dynamically, Label static = Separate Teach-in for backing material and labels, Splice = Learn web material only

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 2 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Material adjustment" index=500 id=V_Abgleich

data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit UInteger |  |  |  |  |  | Dataset | The dataset contains material- and sensor-specific parameters; if the dataset does not match the sensor, the function of the sensor can not be ensured and a notificati-on event is triggered.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Temperature" index=2000 id=V_DiagnoseTemperatur

data type: 16-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 16-bit Integer | -560..1560 | 200 |  |  |  | Sensor temperature |

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 1 | 1 |
element bit | 15 - 8 | 7 - 0 |

## Variable "Measurement" index=2001 id=V_DiagnoseBetriebszustand

data type: 40-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 16-bit UInteger | 30..195 | 30 |  |  |  | Cycletime in SIO mode |
2 | 8 | 16-bit UInteger | 400..13000 | 400 |  |  |  | Cycletime in IO-Link mode |
3 | 0 | 8-bit UInteger |  |  |  |  |  | Quality of the last Teach-in |

octet | 0 | 1 | 2 | 3 | 4 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 2 | 2 | 3 |
element bit | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "Measurement data channel description" index=16512 id=V_MDCDescriptor

data type: 88-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 56 | 32-bit Integer |  | 0 |  |  |  | Lower limit | Lower limit of the measuring range
2 | 24 | 32-bit Integer |  | 1023 |  |  |  | Upper limit | Upper limit of the measuring range
3 | 8 | 16-bit Integer |  | 0 |  |  |  | Unit code |
4 | 0 | 8-bit Integer |  | -1 |  |  |  | Scale | Process data value * (10 ^ scale) [Unit code] = measuring value

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 4 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
16384 (0x4000) | Error | Temperature fault | Overload
16912 (0x4210) | Warning | Device temperature over-run | Clear source of heat
16928 (0x4220) | Warning | Device temperature under-run | Insulate device
36000 (0x8ca0) | Notification | Manual Teach-in not successful | Manual Teach-in process was not successful.
36001 (0x8ca1) | Notification | Manual Teach-in successful | Manual Teach-in process was successful.
36003 (0x8ca3) | Warning | Material adjustment data record does not match the sensor | The material adjustment dataset does not match the sensor. Please execute a Teach-in.
36004 (0x8ca4) | Warning | Manual Teach-in is executed | The sensor can not be used because of a running button or pin 5 teach-in.

[Top]

## Process Data Formatting

Formatting for Process Data id=PI_ProcessDataIn
Subindex 1: * 0.1 + 0 Dec.1
Subindex 2: * 1 + 0 Dec.0
Subindex 3:
Subindex 4:
Subindex 5:

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag, ro

Observation Menu
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSC1Param.SP1 * 0.1 + 0, ro Dec.1
V_SSC1Param.SP2 * 0.1 + 0, ro Dec.1
V_SSC1Config.Logic, ro
V_SSC1Config.Mode, ro
V_SSC1AdvancedConfig.Switch-off delay, ro Dec.0
SSC2: switch signal channel 2 - pin 2 (pnp)
V_SSC2Param.SP1 * 0.1 + 0, ro Dec.1
V_SSC2Param.SP2 * 0.1 + 0, ro Dec.1
V_SSC2Config.Logic, ro
V_SSC2Config.Mode, ro
V_SSC2AdvancedConfig.Switch-off delay, ro Dec.0
Material adjustment
V_Abgleich.Dataset, ro Hex
Temperature compensation
V_TempKomp.Mode, ro
Synchronisation
V_SyncMux.Mode, ro
User interface
V_BedienungEingabe.Teach-in input, ro
V_BedienungEingabe.Manual Teach-in method, ro
V_BedienungAusgabe.Mode, ro
V_BedienungFeedback.Mode, ro
Measurement data channel description
V_MDCDescriptor.Lower limit * 0.1 + 0, ro Dec.1
V_MDCDescriptor.Upper limit * 0.1 + 0, ro Dec.1
V_MDCDescriptor.Unit code, ro
V_MDCDescriptor.Scale, ro
ProcessDataInput
V_ProcessDataInput.1 * 0.1 + 0, ro Dec.1
V_ProcessDataInput.2, ro Dec.0
V_ProcessDataInput.3, ro
V_ProcessDataInput.4, ro
V_ProcessDataInput.5, ro

Diagnosis Menu
Sensor diagnosis
V_DiagnoseTemperatur.Sensor temperature * 0.1 + 0 °C, ro Dec.1
Measurement diagnosis
V_DiagnoseBetriebszustand.Cycletime in SIO mode * 0.01 + 0 ms, ro Dec.3
V_DiagnoseBetriebszustand.Cycletime in IO-Link mode * 0.01 + 0 ms, ro Dec.3
V_DiagnoseBetriebszustand.Quality of the last Teach-in, ro
Device Status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag, rw

Parameter Menu
Teach-in channel
V_TeachInChannel, rw
V_TeachInStatus, ro
V_SystemCommand, Button:=75
V_SystemCommand, Button:=76
V_SystemCommand, Button:=79
V_TeachInKonfig.Splice threshold + 0 %, rw Dec.1
V_TeachInKonfig.Teach-in type, rw
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSC1Param.SP1 * 0.1 + 0, rw Dec.1
V_SSC1Param.SP2 * 0.1 + 0, rw Dec.1
V_SSC1Config.Logic, rw
V_SSC1Config.Mode, rw
V_SSC1AdvancedConfig.Switch-off delay, rw Dec.0
SSC2: switch signal channel 2 - pin 2 (pnp)
V_SSC2Param.SP1 * 0.1 + 0, rw Dec.1
V_SSC2Param.SP2 * 0.1 + 0, rw Dec.1
V_SSC2Config.Logic, rw
V_SSC2Config.Mode, rw
V_SSC2AdvancedConfig.Switch-off delay, rw Dec.0
Material adjustment
V_Abgleich.Dataset, rw Hex
Temperature compensation
V_TempKomp.Mode, rw
Synchronisation
V_SyncMux.Mode, rw
User interface
V_BedienungEingabe.Teach-in input, rw
V_BedienungEingabe.Manual Teach-in method, rw
V_BedienungAusgabe.Mode, rw
V_BedienungFeedback.Mode, rw
System command
V_SystemCommand, Button:=130
Device access locks
V_DeviceAccessLocks.Parameter (write) Access Lock, rw
V_DeviceAccessLocks.Local Parameterization Lock, rw
V_DeviceAccessLocks.Local User Interface Lock, rw

Observation Menu
Measurement data channel description
V_MDCDescriptor.Lower limit * 0.1 + 0, ro Dec.1
V_MDCDescriptor.Upper limit * 0.1 + 0, ro Dec.1
V_MDCDescriptor.Unit code, ro
V_MDCDescriptor.Scale, ro
ProcessDataInput
V_ProcessDataInput.1 * 0.1 + 0, ro Dec.1
V_ProcessDataInput.2, ro Dec.0
V_ProcessDataInput.3, ro
V_ProcessDataInput.4, ro
V_ProcessDataInput.5, ro

Diagnosis Menu
Sensor diagnosis
V_DiagnoseTemperatur.Sensor temperature * 0.1 + 0 °C, ro Dec.1
Measurement diagnosis
V_DiagnoseBetriebszustand.Cycletime in SIO mode * 0.01 + 0 ms, ro Dec.3
V_DiagnoseBetriebszustand.Cycletime in IO-Link mode * 0.01 + 0 ms, ro Dec.3
V_DiagnoseBetriebszustand.Quality of the last Teach-in, ro
Device Status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag, rw

Parameter Menu
Teach-in channel
V_TeachInChannel, rw
V_TeachInStatus, ro
V_SystemCommand, Button:=75
V_SystemCommand, Button:=76
V_SystemCommand, Button:=79
V_TeachInKonfig.Splice threshold + 0 %, rw Dec.1
V_TeachInKonfig.Teach-in type, rw
SSC1: switch signal channel 1 - pin 4 (push-pull)
V_SSC1Param.SP1 * 0.1 + 0, rw Dec.1
V_SSC1Param.SP2 * 0.1 + 0, rw Dec.1
V_SSC1Config.Logic, rw
V_SSC1Config.Mode, rw
V_SSC1AdvancedConfig.Switch-off delay, rw Dec.0
SSC2: switch signal channel 2 - pin 2 (pnp)
V_SSC2Param.SP1 * 0.1 + 0, rw Dec.1
V_SSC2Param.SP2 * 0.1 + 0, rw Dec.1
V_SSC2Config.Logic, rw
V_SSC2Config.Mode, rw
V_SSC2AdvancedConfig.Switch-off delay, rw Dec.0
Material adjustment
V_Abgleich.Dataset, rw Hex
Temperature compensation
V_TempKomp.Mode, rw
Synchronisation
V_SyncMux.Mode, rw
User interface
V_BedienungEingabe.Teach-in input, rw
V_BedienungEingabe.Manual Teach-in method, rw
V_BedienungAusgabe.Mode, rw
V_BedienungFeedback.Mode, rw
System command
V_SystemCommand, Button:=130
Device access locks
V_DeviceAccessLocks.Parameter (write) Access Lock, rw
V_DeviceAccessLocks.Local Parameterization Lock, rw
V_DeviceAccessLocks.Local User Interface Lock, rw

Observation Menu
Measurement data channel description
V_MDCDescriptor.Lower limit * 0.1 + 0, ro Dec.1
V_MDCDescriptor.Upper limit * 0.1 + 0, ro Dec.1
V_MDCDescriptor.Unit code, ro
V_MDCDescriptor.Scale, ro
ProcessDataInput
V_ProcessDataInput.1 * 0.1 + 0, ro Dec.1
V_ProcessDataInput.2, ro Dec.0
V_ProcessDataInput.3, ro
V_ProcessDataInput.4, ro
V_ProcessDataInput.5, ro

Diagnosis Menu
Sensor diagnosis
V_DiagnoseTemperatur.Sensor temperature * 0.1 + 0 °C, ro Dec.1
Measurement diagnosis
V_DiagnoseBetriebszustand.Cycletime in SIO mode * 0.01 + 0 ms, ro Dec.3
V_DiagnoseBetriebszustand.Cycletime in IO-Link mode * 0.01 + 0 ms, ro Dec.3
V_DiagnoseBetriebszustand.Quality of the last Teach-in, ro
Device Status
V_ErrorCount
V_DeviceStatus
V_DetailedDeviceStatus

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.